10T Right-hand Drive Four-Wheel Drive chassis
Chassis Brief configuration:
Cab: Single row, right-hand drive, 2080mm wide
Wheelbase: 3390mm
Chassis dimensions: 6080*2170*2580mm
Drive configuration: 4*4
Engine: Yunnei YN38CRD1, inline four-cylinder, 3.76L displacement, China IV emission standard, 95kw, 365N.M
Transmission: Fast 6DSX60T (6-speed manual)
Front axle: 2.7T, drum type (four-wheel drive front axle)
Rear axle: 5.5T, drum axle, 4.33 gear ratio
Frame: 188 double layer * 800mm, straight beam
Leaf springs: 8/10+7
Tires: 245/70R19.5 or 8.25R20, 6+1 tires
Transfer case: Hubei Senyu
Low voltage platform: 24V
Fuel tank: 90L iron
Braking: Air brakes, exhaust brakes, exhaust brakes, ABS
Other features: Air conditioning (heating and cooling), power windows, multi-function steering wheel
Front/rear track: 1760/1630mm
Chassis front/rear overhang: 1265/1425mm
Chassis approach angle/departure angle: 25°/18°
Minimum ground clearance: 200mm
Vehicles that can be modified : logistics vehicles, sanitation vehicles , etc.
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